**BAB 1**

**SURAT AKUAN PENYEBUTHARGA**

**LEMBAGA PEMBANGUNAN PELABURAN MALAYSIA**

**TINGKAT 14, MIDA SENTRAL**

**NO. 5, JALAN STESEN SENTRAL 5**

**KUALA LUMPUR SENTRAL**

**50470 KUALA LUMPUR**

**SEBUTHARGA MIDA BIL. 12/2025**

**SEBUTHARGA PERKHIDMATAN PENGGANTIAN VIDEO WALL DI LOBI BANGUNAN MIDA SENTRAL**

Kepada:

Penyebutharga-penyebutharga,

**Borang ini hendaklah dikembalikan bersama-sama dengan DOKUMEN MAKLUMBALAS TEKNIKAL DAN JADUAL HARGA di dalam SAMPUL SURAT BERLAKRI**

**SURAT AKUAN PENYEBUTHARGA**

**Kepada:**

**Ketua Pegawai Eksekutif**

**Lembaga Pembangunan Pelaburan Malaysia**

**MIDA Sentral**

**No. 5, Jalan Stesen Sentral 5**

**Kuala Lumpur Sentral**

**50470 Kuala Lumpur**

Tuan,

**SEBUTHARGA MIDA BIL: 12/2025**

**SEBUTHARGA** **PERKHIDMATAN PENGGANTIAN VIDEO WALL DI LOBI BANGUNAN MIDA SENTRAL** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Di bawah dan tertakluk kepada Arahan Kepada Penyebutharga, saya yang menurunkan tandatangan di bawah ini adalah dengan ini mengambil bahagian sebutharga dan menawarkan untuk melaksanakan perkhidmatan di atas mengikut penentuan spesifikasi yang ditetapkan di dalam Dokumen Sebutharga.

2. Saya yang menurunkan tandatangan di bawah ini bersetuju menerima serta mematuhi dan terikat dengan semua Syarat-syarat Kontrak dan Spesifikasi Sebutharga ini dan bersetuju di atas harga yang ditawarkan RM……….............. sebagai asas perkiraan bagi pembayaran perkhidmatan yang telah dipesan oleh Lembaga Pembangunan Pelaburan Malaysia.

3. Dengan ini juga telah difahami bahawa MIDA berhak menerima atau menolak sebarang sebutharga ini, sama ada harga yang ditawarkan rendah atau tinggi atau sama dengan sebutharga-sebutharga yang lain. Saya juga bersetuju untuk menerima kesemua atau sebahagian dari item-item yang ditawarkan dan sedia mengikut kehendak dan pertimbangan MIDA. Saya juga bersetuju bahawa harga sebutharga yang saya beri ini akan sahlaku (*valid*) dan tidak ditarik balik dalam tempoh sembilan puluh (90) hari dari tarikh tutup sebutharga dan tiada apa-apa syarat dikenakan selepas tarikh ditetapkan.

4.Selanjutnya saya bersetuju sekiranya sebutharga saya diterima, saya akan mengikat perjanjian kontrak serta memberi bon pelaksanaan dalam tempoh empat belas (14) hari dari tarikh terima surat tawaran dari MIDA, sekiranya diarahkan.

5. Saya juga mengesahkan, setelah menyemak sendiri iaitu semua dokumen yang digunakan untuk sebutharga ini adalah yang sebenar yang terdapat di dalam Dokumen Sebutharga.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Nama Penyebutharga | : |  |  |  |
|  |  |  |  | (Tandatangan Penyebutharga) |
| Alamat dan Cop Rasmi Syarikat | : |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Tarikh | : |  |  |  |
|  |  |  |  |  |
| Nama Saksi | : |  |  |  |
|  |  |  |  | (Tandatangan Saksi) |
| Alamat | : |  |  |  |
|  |  |  |  |  |

**SURAT AKUAN PEMBIDA**

**SEBUTHARGA PERKHIDMATAN PERKHIDMATAN PENGGANTIAN VIDEO WALL DI LOBI BANGUNAN MIDA SENTRAL**

**(SEBUTHARGA MIDA NO. 12/2025)**

Saya, ………...………............................................ nombor K.P. …………….................... yang mewakili syarikat ….……………………….…….……………………….................... nombor Pendaftaran syarikat …….…………………................................ dengan ini mengisytiharkan bahawa saya atau mana-mana individu yang mewakili syarikat ini tidak akan menawar atau memberi rasuah kepada mana-mana individu dalam MIDA atau mana-mana individu lain, sebagai sogokan untuk dipilih dalam sebutharga seperti di atas. Bersama ini dilampirkan Surat Perwakilan Kuasa bagi saya mewakili syarikat seperti tercatat di atas untuk membuat pengisytiharan ini.

2. Sekiranya saya, atau mana-mana individu yang mewakili syarikat ini didapati cuba menawar atau memberi rasuah kepada mana-mana individu dalam MIDA atau mana-mana individu lain sebagai sogokan untuk dipilih dalam sebutharga seperti di atas, maka saya sebagai wakil syarikat bersetuju tindakan- tindakan berikut diambil:

2.1 Penarikan balik tawaran kontrak bagi sebutharga di atas; atau

2.2 Penamatan kontrak bagi sebutharga di atas; dan

2.3 Lain-lain tindakan tatatertib mengikut peraturan perolehan Kerajaan yang berkuat-kuasa.

3. Sekiranya terdapat mana-mana individu cuba meminta rasuah daripada saya atau mana-mana individu yang berkaitan dengan syarikat ini sebagai sogokan untuk dipilih dalam sebutharga seperti di atas, maka saya berjanji akan dengan segera melaporkan perbuatan tersebut kepada pejabat Suruhanjaya Pencegahan Rasuah Malaysia (SPRM) atau balai polis yang berhampiran.

Yang Benar,

……….................…………..

Nama :

No. KP :

Cop Syarikat :

**BAB 2 - SPESIFIKASI TEKNIKAL & SKOP KERJA**

| **BIL.** | **PERKHIDMATAN** | **PENERANGAN** | **KUANTITI / LOT** |
| --- | --- | --- | --- |
| **1** | **Display Equipment**  **1.1 LED Video Display** | P2i Normal Indoor LED Display (DP)  SMD  Model: LED-P2.0i-160x80-QL-H  Pixel Pitch: 2.0 mm **(Maximum)**  Brightness: 600 nits  Resolution: 3,040 pixels (W) x 1,680 pixels (H) **(Minimum)**  Total Resolution: Screen Size 5,107,200 pixels  (Metric): Screen Size 6.08m (W) x 3.36m (H) = 20.43 sqm  (Imperial): Module 19.95' (W) x 11.03' (H) = 219.82 sqft  Resolution: Module Size: 160 pixels (W) x 80 pixels (H) 320 mm (W) x 160 mm (H)  Cabinet Type: Magnet Module on Steel Structure  Cabinet Size: Access: 320 mm (W) x 160 mm (H)  Type: Ingress: Front Access  LED Type: RGB 3-in-1 SMD2020  Refresh Rate: 3,840 Hz (Flicker Free)  Colour capability: 281 trillion colours (16-bit+)  Estimated LED Lifetime: 100,000 hours+ **(Mandatory)**  Viewing Angle: 150º horizontal, 140º vertical  Power Consumption: 8,438 watts (maximum) 3,375 watts (average)  Power Phase: 240 VAC / single-phase  Display Weight: 201 kg  Control Software: Asynchronous LED Control System  Display Dimming: 8-bit 256 levels  Calibration: Full depth, LED to LED  LED protection included  Warranty: 3 years on Parts, Software & Labour 4-8 Same business day support  **Note: *Any specification brand or model that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Unit |
| **1.2 Electrical & Signal**  **Cabling Works \*Day Work** | - To supply 25A 3-phase LED Distribution Board come with MCCB, ELCB, MCB and timer contactor.  - To supply and install incoming power to LED Distribution Board (est. up to 20m length)  - To supply and install outgoing electrical cables from electrical distribution board to LED panels (est. up to 10m length)  - To supply and install outgoing CAT6 cables from Video Processor (Control room) to LED panels (est. up to 15m length)  - To terminate all power & network cables for all LED panels.  **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |
| **1.3 LED Display Mounting and Installation Works**  **\*Day Work** | * To supply and install a wall-mounted simplified front access LED display structure. * To supply labour and equipment and to dismantle existing videowall and frame and recycle/disposal. * Installation of LED panels inclusive of mounting, hanging, lifting, etc.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |
| **1.4 LED Display Control System** | * To supply and install All-in-One LED Video Media Player. * To supply and install LED Control System software * To supply and install 4x4 Seamless Matrix Switcher.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |
| **2** | **Sound System** | * To supply Six (6) units Full Range ceiling mounted speakers. * To supply DSPPA DMA6500U 500W 6 Zones Mixer Amplifier c/w USB, Bluetooth and FM. * To supply and install IVA U5200-H2 come with two (2) Wireless Handheld microphone. * To supply and install 12U wall mounted server rack. * To supply and install speaker cables from mixer amplifier to speakers 8meters height (est. up to 80m length). * To supply speaker testing and commissioning.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |
| **3** | **Static Live Feed** | * To supply and install the following items as below: * 4K POE PTZ Camera x 3 units PTZ Controller with joystick. * 4CH HDMI Video Switcher come with 10.1InchFHD IPS LCD display. * Live Stream Switcher. * Dual HDMI to USB-C Video Capture * Complete installation, termination, Cabling running uPVC conduit in surface mount with all necessary accessories & connectors. Complete system testing & commissioning come with training.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |
| **4** | **Content Manager** | * To supply Digital Signage Content Management Systems * Digital Signage CMS (Software) * Type: Cloud-based or HybridCore Features: * Multi-zone layout (video, clock, image, ticker, live feed) including space for content to be uploaded as advertisement * Support for RTMP, YouTube Live, IP camera stream * Content scheduling, proof-of-play reporting * User permissions, audit trail, remote access * Mobile and web dashboard * Support: * Minimum 5 years licence/support included * Free CMS & OS upgrades, 24/7 support access * Network Infrastructure * Wired Ethernet (preferred), Wi-Fi as backup * Router with QoS and remote management * Optional 4G/5G modem for redundancy * Free user training   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** |  |
| **5** | **Project Management** | * Complete testing and commissioning * Project Management & Consultancy * Project Insurance * User training and User Manual on Live Event Streaming, LED display operation.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | Lot |
| **6** | **Presentation**  **(if required)** | * Participants will be required to present their proposal in person or via online briefing, including a Q&A session. * Presentation must include:  1. Technical Proposal  * Full solution architecture and system layout * List of hardware and software with model numbers and specifications * Integration details for CMS, MCP, live feed, audio, touchscreen tablet, etc. * Network and power requirements  1. Value-Added Services  * Installation, setup, and configuration plan * Training sessions and materials * Content design or starter media templates * Preventive maintenance schedule * Spare units or hot-swap policy * Warranty and service levels (minimum 3+2 years)  1. Implementation Plan  * Project timeline with key milestones * Dismantle, recycle/disposal and delivery and installation timeline * Testing and commissioning procedure  1. Support & Escalation  * Warranty scope and response times * Support contact details and escalation process * Software update/upgrade policy  1. Commercial Proposal  * Detailed cost breakdown (itemised) * Optional add-ons and pricing * Terms & conditions, payment schedule |  |
| **7** | **Warranty** | * Warranty & Support Summary * Minimum Warranty: 3 years on all hardware/software * Support SLA: * Remote diagnosis within 24 hours * On-site resolution within 48-72 hours * Replacement Clause: * Unserviceable items during warranty must be replace within 5 working days * Replaced item must be of equal or higher spec/value * Hot-swap/loan units to be provided for delays * To provide preventive maintenance within the warranty period. |  |
| **8** | **Value Added** | * Additional warranty 2 years * Cloud storage restoration * Interactive Touchscreen Tablet * Login to CMS dashboard and drag/drop content live * Switch between event layouts or signage playlists * Control media zones with touch presets   (via MCP software)   * Collaborative whiteboard or annotation tool   (built-in apps)   * Free stylus or writing tool * Spare units or hot-swap policy |  |

**BAB 3 – JADUAL MAKLUMBALAS TEKNIKAL**

| **BIL.** | **PERKHIDMATAN** | **PENERANGAN** | **KUANTITI / LOT** | **MAKLUM BALAS** |
| --- | --- | --- | --- | --- |
| **1** | **Display Equipment**  **1.1 LED Video Display** | P2i Normal Indoor LED Display (DP)  SMD  Model: LED-P2.0i-160x80-QL-H  Pixel Pitch: 2.0 mm **(Maximum)**  Brightness: 600 nits  Resolution: 3,040 pixels (W) x 1,680 pixels (H) **(Minimum)**  Total Resolution: Screen Size 5,107,200 pixels  (Metric): Screen Size 6.08m (W) x 3.36m (H) = 20.43 sqm  (Imperial): Module 19.95' (W) x 11.03' (H) = 219.82 sqft  Resolution: Module Size: 160 pixels (W) x 80 pixels (H) 320 mm (W) x 160 mm (H)  Cabinet Type: Magnet Module on Steel Structure  Cabinet Size: Access: 320 mm (W) x 160 mm (H)  Type: Ingress: Front Access  LED Type: RGB 3-in-1 SMD2020  Refresh Rate: 3,840 Hz (Flicker Free)  Colour capability: 281 trillion colours (16-bit+)  Estimated LED Lifetime: 100,000 hours+ **(Mandatory)**  Viewing Angle: 150º horizontal, 140º vertical  Power Consumption: 8,438 watts (maximum) 3,375 watts (average)  Power Phase: 240 VAC / single-phase  Display Weight: 201 kg  Control Software: Asynchronous LED Control System  Display Dimming: 8-bit 256 levels  Calibration: Full depth, LED to LED  LED protection included  Warranty: 3 years on Parts, Software & Labour 4-8 Same business day support  **Note: *Any specification brand or model that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Unit |  |
| **1.2 Electrical & Signal**  **Cabling Works \*Day Work** | - To supply 25A 3-phase LED Distribution Board come with MCCB, ELCB, MCB and timer contactor.  - To supply and install incoming power to LED Distribution Board (est. up to 20m length)  - To supply and install outgoing electrical cables from electrical distribution board to LED panels (est. up to 10m length)  - To supply and install outgoing CAT6 cables from Video Processor (Control room) to LED panels (est. up to 15m length)  - To terminate all power & network cables for all LED panels.  **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |  |
| **1.3 LED Display Mounting and Installation Works**  **\*Day Work** | * To supply and install a wall-mounted simplified front access LED display structure. * To supply labour and equipment and to dismantle existing videowall and frame and recycle/disposal. * Installation of LED panels inclusive of mounting, hanging, lifting, etc.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |  |
| **1.4 LED Display Control System** | * To supply and install All-in-One LED Video Media Player. * To supply and install LED Control System software * To supply and install 4x4 Seamless Matrix Switcher.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |  |
| **2** | **Sound System** | * To supply Six (6) units Full Range ceiling mounted speakers. * To supply DSPPA DMA6500U 500W 6 Zones Mixer Amplifier c/w USB, Bluetooth and FM. * To supply and install IVA U5200-H2 come with two (2) Wireless Handheld microphone. * To supply and install 12U wall mounted server rack. * To supply and install speaker cables from mixer amplifier to speakers 8meters height (est. up to 80m length). * To supply speaker testing and commissioning.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |  |
| **3** | **Static Live Feed** | * To supply and install the following items as below: * 4K POE PTZ Camera x 3 units PTZ Controller with joystick. * 4CH HDMI Video Switcher come with 10.1InchFHD IPS LCD display. * Live Stream Switcher. * Dual HDMI to USB-C Video Capture * Complete installation, termination, Cabling running uPVC conduit in surface mount with all necessary accessories & connectors. Complete system testing & commissioning come with training.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |  |
| **4** | **Content Manager** | * To supply Digital Signage Content Management Systems * Digital Signage CMS (Software) * Type: Cloud-based or HybridCore Features: * Multi-zone layout (video, clock, image, ticker, live feed) including space for content to be uploaded as advertisement * Support for RTMP, YouTube Live, IP camera stream * Content scheduling, proof-of-play reporting * User permissions, audit trail, remote access * Mobile and web dashboard * Support: * Minimum 5 years licence/support included * Free CMS & OS upgrades, 24/7 support access * Network Infrastructure * Wired Ethernet (preferred), Wi-Fi as backup * Router with QoS and remote management * Optional 4G/5G modem for redundancy * Free user training   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** |  |  |
| **5** | **Project Management** | * Complete testing and commissioning * Project Management & Consultancy * Project Insurance * User training and User Manual on Live Event Streaming, LED display operation.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | Lot |  |
| **6** | **Presentation**  **(if required)** | * Participants will be required to present their proposal in person or via online briefing, including a Q&A session. * Presentation must include:  1. Technical Proposal  * Full solution architecture and system layout * List of hardware and software with model numbers and specifications * Integration details for CMS, MCP, live feed, audio, touchscreen tablet, etc. * Network and power requirements  1. Value-Added Services  * Installation, setup, and configuration plan * Training sessions and materials * Content design or starter media templates * Preventive maintenance schedule * Spare units or hot-swap policy * Warranty and service levels (minimum 3+2 years)  1. Implementation Plan  * Project timeline with key milestones * Dismantle, recycle/disposal and delivery and installation timeline * Testing and commissioning procedure  1. Support & Escalation  * Warranty scope and response times * Support contact details and escalation process * Software update/upgrade policy  1. Commercial Proposal  * Detailed cost breakdown (itemised) * Optional add-ons and pricing * Terms & conditions, payment schedule |  |  |
| **7** | **Warranty** | * Warranty & Support Summary * Minimum Warranty: 3 years on all hardware/software * Support SLA: * Remote diagnosis within 24 hours * On-site resolution within 48-72 hours * Replacement Clause: * Unserviceable items during warranty must be replace within 5 working days * Replaced item must be of equal or higher spec/value * Hot-swap/loan units to be provided for delays * To provide preventive maintenance within the warranty period. |  |  |
| **8** | **Value Added** | * Additional warranty 2 years * Cloud storage restoration * Interactive Touchscreen Tablet * Login to CMS dashboard and drag/drop content live * Switch between event layouts or signage playlists * Control media zones with touch presets   (via MCP software)   * Collaborative whiteboard or annotation tool   (built-in apps)   * Free stylus or writing tool * Spare units or hot-swap policy |  |  |

**BAB 4 - KETERANGAN MENGENAI KAKITANGAN & PENGALAMAN SYARIKAT**

1. **PENGALAMAN/PROFIL SYARIKAT**

Senarai projek yang sama yang telah disiapkan dalam tempoh tiga tahun terakhir mengikut kronologi:-

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **No.** | **Butiran Kontrak** | **Nama Pelanggan**  **dan Alamat** | **Jumlah**  **Kontrak (RM)** | **Tarikh Siap** |
|  |  |  |  |  |

1. **PROJEK YANG SEDANG DILAKSANAKAN**

Senarai projek:-

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **No.** | **Butiran Kontrak** | **Nama Pelanggan & Alamat** | **Jumlah Kontrak (RM)** | **Tarikh Mula** | **Tarikh Dijangka Siap** | **% Kemajuan** |
|  |  |  |  |  |  |  |

**BAB 5 – JADUAL MAKLUMBALAS HARGA**

| **BIL.** | **PERKHIDMATAN** | **PENERANGAN** | **KUANTITI / LOT** | **HARGA/ UNIT (RM)** | **HARGA (RM)** |
| --- | --- | --- | --- | --- | --- |
| **1** | **Display Equipment**  **1.1 LED Video Display** | P2i Normal Indoor LED Display (DP)  SMD  Model: LED-P2.0i-160x80-QL-H  Pixel Pitch: 2.0 mm **(Maximum)**  Brightness: 600 nits  Resolution: 3,040 pixels (W) x 1,680 pixels (H) **(Minimum)**  Total Resolution: Screen Size 5,107,200 pixels  (Metric): Screen Size 6.08m (W) x 3.36m (H) = 20.43 sqm  (Imperial): Module 19.95' (W) x 11.03' (H) = 219.82 sqft  Resolution: Module Size: 160 pixels (W) x 80 pixels (H) 320 mm (W) x 160 mm (H)  Cabinet Type: Magnet Module on Steel Structure  Cabinet Size: Access: 320 mm (W) x 160 mm (H)  Type: Ingress: Front Access  LED Type: RGB 3-in-1 SMD2020  Refresh Rate: 3,840 Hz (Flicker Free)  Colour capability: 281 trillion colours (16-bit+)  Estimated LED Lifetime: 100,000 hours+ **(Mandatory)**  Viewing Angle: 150º horizontal, 140º vertical  Power Consumption: 8,438 watts (maximum) 3,375 watts (average)  Power Phase: 240 VAC / single-phase  Display Weight: 201 kg  Control Software: Asynchronous LED Control System  Display Dimming: 8-bit 256 levels  Calibration: Full depth, LED to LED  LED protection included  Warranty: 3 years on Parts, Software & Labour 4-8 Same business day support  **Note: *Any specification brand or model that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Unit |  |  |
| **1.2 Electrical & Signal**  **Cabling Works \*Day Work** | - To supply 25A 3-phase LED Distribution Board come with MCCB, ELCB, MCB and timer contactor.  - To supply and install incoming power to LED Distribution Board (est. up to 20m length)  - To supply and install outgoing electrical cables from electrical distribution board to LED panels (est. up to 10m length)  - To supply and install outgoing CAT6 cables from Video Processor (Control room) to LED panels (est. up to 15m length)  - To terminate all power & network cables for all LED panels.  **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |  |  |
| **1.3 LED Display Mounting and Installation Works**  **\*Day Work** | * To supply and install a wall-mounted simplified front access LED display structure. * To supply labour and equipment and to dismantle existing videowall and frame and recycle/disposal. * Installation of LED panels inclusive of mounting, hanging, lifting, etc.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |  |  |
| **1.4 LED Display Control System** | * To supply and install All-in-One LED Video Media Player. * To supply and install LED Control System software * To supply and install 4x4 Seamless Matrix Switcher.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |  |  |
| **2** | **Sound System** | * To supply Six (6) units Full Range ceiling mounted speakers. * To supply DSPPA DMA6500U 500W 6 Zones Mixer Amplifier c/w USB, Bluetooth and FM. * To supply and install IVA U5200-H2 come with two (2) Wireless Handheld microphone. * To supply and install 12U wall mounted server rack. * To supply and install speaker cables from mixer amplifier to speakers 8meters height (est. up to 80m length). * To supply speaker testing and commissioning.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |  |  |
| **3** | **Static Live Feed** | * To supply and install the following items as below: * 4K POE PTZ Camera x 3 units PTZ Controller with joystick. * 4CH HDMI Video Switcher come with 10.1InchFHD IPS LCD display. * Live Stream Switcher. * Dual HDMI to USB-C Video Capture * Complete installation, termination, Cabling running uPVC conduit in   surface mount with all necessary accessories & connectors.  Complete system testing & commissioning come with training.  **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | 1 Lot |  |  |
| **4** | **Content Manager** | * To supply Digital Signage Content Management Systems * Digital Signage CMS (Software) * Type: Cloud-based or HybridCore Features: * Multi-zone layout (video, clock, image, ticker, live feed) including space for content to be uploaded as advertisement * Support for RTMP, YouTube Live, IP camera stream * Content scheduling, proof-of-play reporting * User permissions, audit trail, remote access * Mobile and web dashboard * Support: * Minimum 5 years licence/support included * Free CMS & OS upgrades, 24/7 support access * Network Infrastructure * Wired Ethernet (preferred), Wi-Fi as backup * Router with QoS and remote management * Optional 4G/5G modem for redundancy * Free user training   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** |  |  |  |
| **5** | **Project Management** | * Complete testing and commissioning * Project Management & Consultancy * Project Insurance * User training and User Manual on Live Event Streaming, LED display operation.   **Note: *Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.*** | Lot |  |  |
| **6** | **Presentation**  **(if required)** | * Participants will be required to present their proposal in person or via online briefing, including a Q&A session. * Presentation must include:  1. Technical Proposal  * Full solution architecture and system layout * List of hardware and software with model numbers and specifications * Integration details for CMS, MCP, live feed, audio, touchscreen tablet, etc. * Network and power requirements  1. Value-Added Services  * Installation, setup, and configuration plan * Training sessions and materials * Content design or starter media templates * Preventive maintenance schedule * Spare units or hot-swap policy * Warranty and service levels (minimum 3+2 years)  1. Implementation Plan  * Project timeline with key milestones * Dismantle, recycle/disposal and delivery and installation timeline * Testing and commissioning procedure  1. Support & Escalation  * Warranty scope and response times * Support contact details and escalation process * Software update/upgrade policy  1. Commercial Proposal  * Detailed cost breakdown (itemised) * Optional add-ons and pricing * Terms & conditions, payment schedule |  |  |  |
| **7** | **Warranty** | * Warranty & Support Summary * Minimum Warranty: 3 years on all hardware/software * Support SLA: * Remote diagnosis within 24 hours * On-site resolution within 48-72 hours * Replacement Clause: * Unserviceable items during warranty must be replace within 5 working days * Replaced item must be of equal or higher spec/value * Hot-swap/loan units to be provided for delays * To provide preventive maintenance within the warranty period. |  |  |  |
| **8** | **Value Added** | * Additional warranty 2 years * Cloud storage restoration * Interactive Touchscreen Tablet * Login to CMS dashboard and drag/drop content live * Switch between event layouts or signage playlists * Control media zones with touch presets   (via MCP software)   * Collaborative whiteboard or annotation tool   (built-in apps)   * Free stylus or writing tool * Spare units or hot-swap policy |  |  |  |
| **Jumlah (RM)** | | | | |  |
| ***Sales & Service Tax (SST 8%)* sekiranya ada** | | | | |  |
| **Jumlah keseluruhan termasuk SST 8%** | | | | |  |

**BAB 6**

**BUTIR-BUTIR PENYEBUTHARGA & MAKLUMAT KEWANGAN SYARIKAT**

Syarikat perlu mengisi dengan lengkap semua seksyen dalam borang ini. Sekiranya ruang tidak mencukupi, maklumat boleh dikemukakan dalam kertas berasingan.

1. **MAKLUMAT AM**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | Nama Syarikat | | | : |  | | |
|  | Alamat | | | : |  | | |
|  | No. Telefon | | | : |  | | |
|  | No. Faks | | | : |  | | |
|  | Emel | | | : |  | | |
|  | Tarikh Pendaftaran / Penubuhan | | | : |  | | |
|  | No. Daftar Syarikat / Perniagaan | | | : |  | | |
|  | Tempat Pendaftaran/ Penubuhan | | | : |  | | |
|  | Komposisi Pemegang Saham | | | : |  | | |
| **No.** | **Nama Pemegang Saham** | | | **Jawatan** | **% Pegangan** | |
|  |  | | |  |  | |

* 1. Peratusan Penyertaan Bumiputera : \_\_\_\_\_\_\_\_ (%). (Sila kemukakan maklumat lanjut atau salinan sah pendaftaran sebagai Pembekal Bumiputera dengan Kementerian Kewangan).
  2. Maklumat Pendaftaran Kementerian Kewangan

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **No.** | **No. Pendaftaran** | **No. bidang** | **Butiran / Keterangan** | **Tempoh Sah** |
|  |  |  |  |  |
|  |  |  |  |  |

Nota : Sila lampirkan salinan sijil pendaftaran.

* 1. Struktur Modal Syarikat :

|  |  |
| --- | --- |
| 1. Modal Dibenarkan | : |
| 1. Modal Berbayar | : |

**B. KEWANGAN**

a. Ringkasan aset dan tanggungan berdasarkan akaun yang diaudit bagi tiga (3) tahun terakhir.

|  |  |  |  |
| --- | --- | --- | --- |
| **Tahun Kewangan:** | **2022 (RM)** | **2023**  **(RM)** | **2024**  **(RM)** |
| * Jumlah Aset * Aset Semasa * Jumlah Tanggungan * Tanggungan Semasa * Nilai Bersih * Modal Kerja |  |  |  |

* + 1. Bank-bank Utama:

|  |  |  |
| --- | --- | --- |
| **No.** | **Nama Bank & Alamat** | **Jenis Akaun** |
| 1.  2.  3. |  |  |

* + 1. Kemudahan Kredit (Jenis dan jumlah kredit yang boleh disediakan oleh syarikat:)

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Jenis Kemudahan Kredit** | **Bank/Institusi Kewangan** | **Jumlah (RM)** |
| 1.  2.  3. |  |  |  |

**Nota:**

1. **Penyata Kewangan yang telah diaudit bagi tempoh tiga (3) tahun terakhir hendaklah disertakan bersama-sama serahan borang sebutharga.**
2. **Penyata Bank bagi tempoh tiga (3) bulan terakhir hendaklah disertakan bersama-sama serahan borang sebutharga.**

**LAMPIRAN SEMAKAN**

**SEBUTHARGA PERKHIDMATAN PENGGANTIAN VIDEO WALL DI LOBI BANGUNAN MIDA SENTRAL**

**SEBUTHARGA MIDA BIL: 12/2025**

Sila tandakan **( √ )** bagi Dokumen-dokumen yang disertakan.

| **Bil.** | **Perkara / Dokumen** | **Semakan oleh Syarikat** | **Semakan oleh**  **MIDA** |
| --- | --- | --- | --- |
|  | **Surat Akuan Penyebutharga\*** |  |  |
|  | **Surat Akuan Pembida\*** |  |  |
|  | Maklumat Suruhanjaya Syarikat Malaysia (SSM) (Salinan sijil disertakan) |  |  |
| **Berdaftar dengan SSM\*** |  |  |
| 1. No. Sijil Pendaftaran (sila nyatakan) |  |  |
| 1. Tarikh Sijil Pendaftaran (nyatakan) |  |  |
|  | Maklumat pendaftaran dengan Kementerian Kewangan (MOF) (Salinan Sijil Akuan Pendaftaran dengan MOF disertakan) |  |  |
| Syarikat **berdaftar dengan Kementerian Kewangan (MOF)\*** dalam kod bidang berikut (dan tempoh pendaftaran masih berkuatkuasa):   |  |  | | --- | --- | | **020301** | **Perkakas Elektrik dan Aksesori; atau** | | **020302** | **Perkakas Elektronik dan Aksesori; DAN** | | **221304** | **Audio Visual; dan/atau** | | **222601** | **Akustik dan Gelombang; DAN** | | **210103** | **Perisian – membekalkan semua perisian komputer, termasuk sistem pengendalian, pangkalan data, pakej sedia ada, serta penyelenggaraan** | |  |  |
| * + - * 1. No. Sijil Akuan Pendaftaran (nyatakan) |  |  |
| * + - * 1. Tempoh Sahlaku Sijil Pendaftaran (nyatakan) |  |  |
| * + - * 1. Salinan Sijil disertakan |  |  |
| * + - * 1. Sijil Akuan Pendaftaran Bumiputera (jika ada) |  |  |
| * + - * 1. Peratus Penyertaan/Ekuiti Bumiputera (nyatakan, jika ada) |  |  |
| 5. | **Syarikat mengemukakan Sijil Pematuhan Cukai (TCC)\*** |  |  |
| 6. | Jadual Maklumbalas Teknikal *(Hardcopy & Softcopy)* |  |  |
| 7. | Maklumbalas Harga *(Hardcopy & Softcopy)* |  |  |
| 1. Borang Jadual Harga |  |  |
| 1. Penyata Kewangan (yang telah diaudit) untuk 3 tahun terakhir |  |  |
| 1. Penyata Bank untuk 3 bulan terakhir |  |  |
| 8. | Lain-lain – profil syarikat, katalog, pengalaman kerja dan/atau mana-mana yang berkaitan dengan video wall |  |  |
| 9. | **Pengesahan Oleh Syarikat\*** |  |  |

**\*Mandatori**

|  |
| --- |
| **PENGESAHAN OLEH SYARIKAT** |
| Dengan ini saya mengesahkan bahawa saya telah membaca dan memahami semua syarat-syarat dan terma yang dinyatakan di dalam dokumen sebut harga. Semua maklumat yang dikemukakan adalah benar. |
| |  |  |  | | --- | --- | --- | | Tandatangan | : | ..................................................................................... | | Nama | : | ..................................................................................... | | Jawatan | : | ..................................................................................... | | Tarikh | : | ..................................................................................... | |

|  |
| --- |
| **PENGESAHAN OLEH MIDA** |
| Jawatankuasa Penilaian Sebutharga mengesahkan penerimaan dokumen bertanda kecuali bagi perkara bil. .......................................... (jika ada) :- |
| |  |  |  | | --- | --- | --- | | Tandatangan | : | ..................................................................................... | | Nama | : | ..................................................................................... | | Jawatan | : | ..................................................................................... | | Tarikh | : | ..................................................................................... | |