BAB 1

SURAT AKUAN PENYEBUTHARGA


LEMBAGA PEMBANGUNAN PELABURAN MALAYSIA
TINGKAT 14, MIDA SENTRAL
NO. 5, JALAN STESEN SENTRAL 5
KUALA LUMPUR SENTRAL
50470 KUALA LUMPUR


SEBUTHARGA  MIDA  BIL.  19/2026
SEBUTHARGA KERJA-KERJA MENAIKTARAF SISTEM AUDIO VISUAL DI BILIK MESYUARAT JAPAN, TINGKAT 18, MIDA SENTRAL


Kepada:


Penyebutharga-penyebutharga,


Borang ini hendaklah dikembalikan bersama-sama dengan DOKUMEN MAKLUMBALAS TEKNIKAL DAN JADUAL HARGA di dalam SAMPUL SURAT BERLAKRI


SURAT AKUAN PENYEBUTHARGA

Kepada:

Ketua Pegawai Eksekutif
Lembaga Pembangunan Pelaburan Malaysia 
MIDA Sentral
No. 5, Jalan Stesen Sentral 5
Kuala Lumpur Sentral
50470 Kuala Lumpur

Tuan,

SEBUTHARGA MIDA BIL:  19/2026
[bookmark: _heading=h.syxjxdtra48y]SEBUTHARGA KERJA-KERJA MENAIKTARAF SISTEM AUDIO VISUAL DI BILIK MESYUARAT JAPAN, TINGKAT 18, MIDA SENTRAL

Di bawah dan tertakluk kepada Arahan Kepada Penyebutharga, saya yang menurunkan tandatangan di bawah ini adalah dengan ini mengambil bahagian sebutharga dan menawarkan untuk melaksanakan perkhidmatan di atas mengikut penentuan spesifikasi yang ditetapkan di dalam Dokumen Sebutharga.

2.	Saya yang menurunkan tandatangan di bawah ini bersetuju menerima serta mematuhi dan terikat dengan semua Syarat-syarat Kontrak dan Spesifikasi Sebutharga ini dan bersetuju di atas harga yang ditawarkan RM……….............. sebagai asas perkiraan bagi pembayaran perkhidmatan yang telah dipesan oleh Lembaga Pembangunan Pelaburan Malaysia.

3.	Dengan ini juga telah difahami bahawa MIDA berhak menerima atau menolak sebarang sebutharga ini, sama ada harga yang ditawarkan rendah atau tinggi atau sama dengan sebutharga-sebutharga yang lain.  Saya juga bersetuju untuk menerima kesemua atau sebahagian dari item-item yang ditawarkan dan sedia mengikut kehendak dan pertimbangan MIDA.  Saya juga bersetuju bahawa harga sebutharga yang saya beri ini akan sahlaku (valid) dan tidak ditarik balik dalam tempoh sembilan puluh (90) hari dari tarikh tutup sebutharga dan tiada apa-apa syarat dikenakan selepas tarikh ditetapkan.

4.	Selanjutnya saya bersetuju sekiranya sebutharga saya diterima, saya akan mengikat perjanjian kontrak serta memberi bon pelaksanaan dalam tempoh empat belas (14) hari dari tarikh terima surat tawaran dari MIDA, sekiranya diarahkan.

5.	Saya juga mengesahkan, setelah menyemak sendiri iaitu semua dokumen yang digunakan untuk sebutharga ini adalah yang sebenar yang terdapat di dalam Dokumen Sebutharga.


	Nama Penyebutharga
	:
	
	
	

	
	
	
	
	(Tandatangan Penyebutharga)



	Alamat dan Cop Rasmi Syarikat
	:
	
	
	

	
	
	

	
	

	
	
	

	
	

	

Tarikh
	

:
	


	
	

	
	
	

	
	

	

Nama Saksi
	

:
	

	
	

	
	
	

	
	(Tandatangan Saksi)

	Alamat
	:
	
	
	

	
	
	

	
	





SURAT AKUAN PEMBIDA 

SEBUTHARGA KERJA-KERJA MENAIKTARAF SISTEM AUDIO VISUAL DI BILIK MESYUARAT JAPAN, TINGKAT 18, MIDA SENTRAL

(SEBUTHARGA MIDA NO. 19/2026)

Saya, ………...………............................................ nombor K.P. …………….................... yang mewakili syarikat ….……………………….…….……………………….................... nombor Pendaftaran syarikat …….…………………................................ dengan ini mengisytiharkan bahawa saya atau mana-mana individu yang mewakili syarikat ini tidak akan menawar atau memberi rasuah kepada mana-mana individu dalam MIDA atau mana-mana individu lain, sebagai sogokan untuk dipilih dalam sebutharga seperti di atas. Bersama ini dilampirkan Surat Perwakilan Kuasa bagi saya mewakili syarikat seperti tercatat di atas untuk membuat pengisytiharan ini.

2. Sekiranya saya, atau mana-mana individu yang mewakili syarikat ini didapati cuba menawar atau memberi rasuah kepada mana-mana individu dalam MIDA atau mana-mana individu lain sebagai sogokan untuk dipilih dalam sebutharga seperti di atas, maka saya sebagai wakil syarikat bersetuju tindakan- tindakan berikut diambil:

2.1 	Penarikan balik tawaran kontrak bagi sebutharga di atas; atau
2.2 	Penamatan kontrak bagi sebutharga di atas; dan
2.3 	Lain-lain tindakan tatatertib mengikut peraturan perolehan Kerajaan yang berkuat-kuasa.

3. Sekiranya terdapat mana-mana individu cuba meminta rasuah daripada saya atau mana-mana individu yang berkaitan dengan syarikat ini sebagai sogokan untuk dipilih dalam sebutharga seperti di atas, maka saya berjanji akan dengan segera melaporkan perbuatan tersebut kepada pejabat Suruhanjaya Pencegahan Rasuah Malaysia (SPRM) atau balai polis yang berhampiran.

Yang Benar,


……….................…………..
Nama :
No. KP :
Cop Syarikat :


BAB 2 - SPESIFIKASI TEKNIKAL
	
Bil
	
Perkhidmatan

	Penerangan
	
Jenama / Model
	
Kuantiti/Lot

	









1
	Alphal Pro LED Video Display with Chip On Board (COB) Technology

	-	LED Cabinet Size: 640mm x 	480mm
-	Pixel Pitch : 1.538mm
-	Screen Size (WxH): 3.84m x 	1.92m / 12.6ft x 6.3ft
-	Screen Resolution: 2,496 x 1,248 	pixels
-	LED Cabinet Array: 6 × 4 (W × H)
-	Brightness: 600-800 nits
-	Refresh rate: 3840 Hz
-	Maintenance : Front
-	LED Module Spare Unit : 5pcs
Warranty : 3 year	

Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	




Alphalpro
	24 


	







Nos



	


2
	Installation Of LED (Electrical and Civil)



	· To supply and install 30A three-phase electrical distribution board.
· To supply and install outgoing electrical cables from electrical distribution board to LED panels.
· To supply and install outgoing CAT6 cables from Video Processor to LED panels.
· To terminate all power & network cables for all LED panels.
	



N/A
	1

1


1


1 
	Lot

Lot



Lot


Lot

	






3
	Digital Signal Processor & System Integration

	Digital Signal Processor & System Integration camera with 20x Optical Zoom (Creator (CR-PGMIV-C).
· To Supply and install Intgrated Control Processor
· To supply 10.1 inch Wireless Touch Panel Screen Apple Ipad.
· To programmable 10.1 inch Wireless Touch Panel Screen and AP Router.
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	



Creator CR-PGMIV-C

Apple iPad Pro
	



1


1


1







	



Lot


Lot


Lot




	





4
	Project Management
	· Complete testing and commissioning.
· To supply and install all outgoing cables for all devices, inclusive of all cable installation works.
· Project Management & Consultancy.
· Project Insurance.
· User training and User Manual for all installation item.
· Installation, configuration, setup & cabling.
· Tenderers may provide any suggestions that are deemed beneficial to MIDA.
· To relocate the existing camera to another meeting room, including dismantling, reinstallation, configuration, testing, and commissioning works
· User training and User Manual on LED display operation & basic maintenance work.
	
	








1






 
	








Lot

	


5
	LED Display Mounting and Installation Works
	· Supply and install custom-made ceiling-mounted LED display structure. Open ceiling as needed and make good after installation.
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	
	
1






	
Lot

	


6
	LED Display Control System
	· To supply and install All-in-One LED Controller 	and Processor (Novastar VX600-Pro).
· To supply and install LED Control System 	software.
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	


NovaStar VX600- Pro
	1
	



Nos

	













7
	Microphone System
	· To supply and install Full Digital Conference 	Controller Unit. 32bit high-speed DSP processing, audio acoustic feedback suppression, noise elimination. 
· To supply and install Digital conference 	chairman unit built-in 5.5″ wide LCD touch panel and adopts an embedded Linux operating system and is powered by an ARM Cortex-A7 dual-core 1.2 GHz CPU. 
· To supply and install Fully Digital Twisted Pair 	Conference Delegate Unit built-in loudspeaker c/w 415mm aviation connector plug gooseneck 	microphone with double color indicating light, speaking as Red color / Applying as Green color. Support Camera Auto -Tracking System 	function. 
· Full Digital Power Conference Extension 4 Way 	Output Box with RJ45 interfaces. 
· To supply and install CAT6 cable run in PVC conduit.

Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	
Creator CR-DIG5201-A.



Creator CR-DIG5202X3.




Creator CR-CAT5204B.







Creator CR-CAT5200-EXP-S.

	1




1






49








2


1
	
Nos




Nos






Nos








Nos


Lot

	












8
	Camera System
	· To supply and install Camera Auto-tracking Processor which supports 6 camera Max, c/w with USB Output, Multi-View, zoom etc.
·  To supply and install 16x8 4K Matrix Seamless Switcher Chassis as below:
· 4-channel 4K HDBaseT signal seamless input card,Support external POC power supply x3pcs.
· 4-channel 4K HDMI seamless input signal card x1pc.
· 8-channel 4K HDMI seamless output with audio signal card x2pcs. 
· HDMI, USB Type C Panel 4K HDBaseT Transmitter(150m for 1080P @60Hz, or 120m for 4K2K@60Hz 4:4:4).

· HDMI to USB 3.0 Video Capture & Streamer.


· To supply and install PTZ camera wall mount 20x Optical Zoom.
· To supply and install CAT6 cable & HDMI cable.
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	

Creator MID-MAX1616HD.














CR-uCAT DET 4K 86


Magewell USB Capture HDMI Plus.

Creator CR-VX60ASL.
	


1














11



1



3

1
	


Lot














Nos



Nos



Nos

Lot

	
9

	Digital Signal Processor & System Integration
	· To supply and install Digital Audio Mixer.
· Single- Ear Wireless Intercom Headset System 4 Person
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	Allen & Health CQ12T
Hollyland Solidcom SE Wireless

	1 Lot
	

	10

	

Auxilary Display
	· To supply and install 85" Smart TV c/w wall mounted bracket.
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	
Samsung UA85CU8000
	2
	


Nos

	    11
	


Sound System
	· To supply and install 600 W x 4 at 8 Ω, Power Amplifier Build in DSP function (Matrix mixer, 5 – band PEQ, array EQ, band pass, loudspeaker EQ, limiter delay)
	

BOSE PSX1204D
	1
	


Nos

	














12
	
System Integration

	General Requirement
The Contractor shall supply, install, integrate, configure, test, and commission a complete Audio Visual (AV) system for Meeting Room and Hybrid Meeting purposes. The proposed system shall be fully integrated and compatible with the existing AV system and shall operate seamlessly as a unified system.
System Integration with Existing AV System
The Contractor shall ensure full system integration and interoperability between the proposed AV system and the existing AV infrastructure. Integration works shall include all necessary hardware, software, interfaces, cabling, configuration, programming, and control integration to ensure seamless operation without degradation to the existing system performance.

Hybrid Meeting Functionality
The AV system shall support hybrid meeting functionality, enabling simultaneous physical and remote participation via standard video conferencing platforms (e.g. Microsoft Teams, Zoom, WebEx, or equivalent). The system shall provide clear audio, high-quality video, and stable connectivity for both local and remote participants.
Camera & Auto-Tracking System
The system shall be equipped with a live camera system with automatic speaker tracking capability. The camera shall be fully integrated with the existing microphone system to enable accurate auto-tracking based on active microphone detection. Manual override and preset camera positions shall be provided via the control system.
Audio System Integration
The proposed audio system shall be fully integrated with the existing microphone, loudspeaker, and digital signal processing (DSP) systems. Echo cancellation, noise suppression, automatic gain control, and audio mixing shall be configured to ensure optimal audio quality for hybrid meetings.
Control System
A centralized and user-friendly control interface shall be provided to allow seamless operation of all AV functions, including audio control, camera switching, source selection, display control, and hybrid meeting operation. The control system shall integrate with the existing AV control platform where applicable.
Cabling & Infrastructure
The Contractor shall supply and install all necessary outgoing cables for all AV devices, inclusive of complete cable installation works such as routing, containment, labeling, termination, and testing. All cabling works shall comply with relevant standards and best practices.
Testing & Commissioning
Comprehensive testing and commissioning shall be carried out to verify full system functionality, audio-video synchronization, auto-tracking accuracy, signal stability, and overall performance of the integrated AV system for hybrid meeting operations.
Non-Disruption to Existing System
All installation and integration works shall be carried out without disruption to the operation of the existing AV system. Any temporary shutdown or modification shall be subject to prior approval by the Client.
Documentation & Training
The Contractor shall provide complete system documentation, including as-built drawings, configuration settings, and user manuals. User training shall be conducted to ensure effective operation of the AV system for hybrid meetings.
Cost Inclusion
All AV system integration works shall be deemed included in the contract sum. No additional cost shall be borne by the Client for any works related to system integration, configuration, testing, and commissioning.

	
	
	

	





13
	

Warranty



	[bookmark: _Hlk242956245]The Contractor shall provide a workmanship and service warranty for a minimum period of 12, 24 or 36 months commencing from the Date of Practical Completion / System Acceptance.
This warranty shall cover:
	•	Installation defects
	•	Cabling, termination, 		and finishing 	works
	•	System configuration, 		integration, and 			programming errors
	•	System instability 			caused by installation 		or configuration issues.
 
Warranty Support Scope
During the warranty period, the Contractor shall provide:
	•	Technical support 			services.
	•	System inspection and 		troubleshooting.
	•	Repair or replacement 		of defective equipment.
	•	System reconfiguration 		when required.
	•	On-site support at no 		additional cost for 			issues related to the 		scope of work.

Response Time:
	•	Initial response within 		24–48 working hours 		upon receipt of a fault 		report.
	•	Rectification to be 			carried out within a 			reasonable timeframe, 		subject to spare parts 		availability.

Post-Warranty Support
Upon expiry of the warranty period, the Contractor shall:
	•	Offer paid maintenance 		and support services if 		required.
	•	Provide quotations for 		repair or replacement of 		equipment.

	
	
	

	
14
	Value Added
	· Free 65 Inch Smart TV Panel (2 Unit)
	
	
	



1

BAB 3 – JADUAL MAKLUM BALAS TEKNIKAL
 
	[bookmark: _Hlk242799271]Bil
	
Perkhidmatan

	Penerangan
	
Kuantiti/Lot
	
Jenama / Model
	Maklum Balas
(YA / TIDAK)

	1
	LED Video Display with Chip on Board (COB) Technology (LEDCUBE SYSTEM P1.53-6448)

	-	LED Cabinet Size: 640mm x 480mm
-	Pixel Pitch : 1.538mm
-	Screen Size (WxH): 3.84m x 1.92m / 12.6ft x 	6.3ft
-	Screen Resolution: 2,496 x 1,248 pixels
-	LED Cabinet Array: 6 × 4 (W × H)
-	Brightness: 600-800 nits
-	Refresh rate: 3840 Hz
-	Maintenance : Front
-	LED Module Spare Unit : 5pcs
Warranty : 3 year	

Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	24 


	Nos


	
Alphal P1.53-6448-COB












	

	2
	Installation Of LED (Electrical and Civil)
	· To supply and install 30A three-phase electrical distribution board.
· [bookmark: _GoBack]To supply and install outgoing electrical cables from electrical distribution board to LED panels.
· To supply and install outgoing CAT6 cables from Video Processor to LED panels.
· To terminate all power & network cables for all LED panels.
	1 Lot
	
	

	3
	Digital Signal Processor & System Integration
	· Digital Signal Processor & System Integration camera with 20x Optical Zoom (Creator (CR-PGMIV-C).
· To supply 10.1 inch Wireless Touch Panel Screen (Apple Ipad).
· To programmable 10.1 inch Wireless Touch Panel Screen and AP Router.
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	1


1

1





	
Lot


Lot

Lot







	
Creator CR-PGMIV-C

Apple IPAD PRO
	

	4
	Project Management
	· Complete testing and commissioning.
· To supply and install all outgoing cables for all devices, inclusive of all cable installation works.
· Project Management & Consultancy.
· Project Insurance.
· User training and User Manual for all installation item.
· Installation, configuration, setup & cabling.
· Tenderers may provide any suggestions that are deemed beneficial to MIDA.
· To relocate the existing camera to another meeting room, including dismantling, reinstallation, configuration, testing, and commissioning works
· User training and User Manual on LED display operation & basic maintenance work.
	1 
	Lot
	
	

	5
	LED Display Mounting and Installation Works
	· Supply and install custom-made ceiling-mounted LED display structure. Open ceiling as needed and make good after installation.
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	1
	Lot
	
	

	6
	LED Display Control System
	· To supply and install All-in-One LED Controller 	and Processor (Novastar VX600-Pro).
· To supply and install LED Control System 	software (Novastar VX600-Pro)..
	1
	Nos
	
NovaStar VX600-PRO
	

	7
	Microphone System
	· To supply and install Full Digital Conference 	Controller Unit. 32bit high-speed DSP 	processing, audio acoustic feedback 	suppression, noise elimination (Creator CR-	DIG5201-A).
· To supply and install Digital conference 	chairman unit built-in 5.5″ wide LCD touch 	panel and adopts an embedded Linux 	operating system and is powered by an ARM 	Cortex-A7 dual-core 1.2 GHz CPU (Creator CR-	DIG5202X3).
· To supply and install Fully Digital Twisted Pair 	Conference Delegate Unit built-in loudspeaker 	c/w 415mm aviation connector plug gooseneck 	microphone with double color indicating light, 	speaking as Red color / Applying as Green 	color. Support Camera Auto -Tracking System 	function (Creator CR-CAT5204B).
· Full Digital Power Conference Extension 4 Way 	Output Box with RJ45 interfaces (Creator CR-	CAT5200-EXP-S).
· To supply and install CAT6 cable run in PVC 	conduit.
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	1




1






49







2


1
	Nos




Nos






Nos







Nos


Lot
	Creator CR-DIG5201-A



Creator CRDIG5202X3




Creator CR-Cat5204B





Creator CR-Cat5200-EXP-S
	

	8
	Camera System
	· To supply and install Camera Auto-tracking Processor which supports 6 camera Max, c/w with USB Output, Multi-View, zoom etc (Creator MID-MAX1616HD).
· To supply and install 16x8 4K Matrix Seamless Switcher Chassis as below (Creator CR-uCAT DET 4K 86:
	- 4-channel 4K HDBaseT signal seamless input
	card,Support external POC power supply 	x3pcs.
· 4-channel 4K HDMI seamless input signal card x1pc (Magewell USB Capture HDMI Plus).
· 8-channel 4K HDMI seamless output with audio signal card x2pcs (Creator CR-VX60ASL).

· HDMI, USB Type C Panel 4K HDBaseT Transmitter(150m for 1080P @60Hz, or 120m for 4K2K@60Hz 4:4:4).
· HDMI to USB 3.0 Video Capture & Streamer.


· To supply and install PTZ camera wall mount 20x Optical Zoom.
· To supply and install CAT6 cable & HDMI cable. 
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	



1











11


1


3

1
	



Lot











Nos


Nos


Nos

Lot
	



Creator MID-MAX1616HD









Creator-uCAT DET 4K 86

Magewell Capture HDMI Plus
Creator CR-VX60ASL









	

	9
	Digital Signal Processor & System Integration
	·  To supply and install Digital Audio Mixer (Allen & Health CQ12T).
· Single- Ear Wireless Intercom Headset System (5 Unit).
	1
	Lot
	

Allen & Health CQ12T

	

	10
	Auxilary Display
	· To supply and install 85" Smart TV c/w wall mounted bracket (Samsung UA85CU8000).
	2
	Nos
	
Samsung UA85CU800
	

	11
	Sound / Speaker
	· To Supply and install 600 W x 4 at 8 Ω, Power Amplifier Build in DSP function (Matrix mixer, 5-band PEQ, array EQ, brand pass, Loudspeaker EQ, limiter delay).
· To supply and install 60W 5.25” Ceiling Loudspeaker.
· To supply and install 8 nos 46/0.20mm full copper speaker cable run-in PVC Conduit.
	1



8


1
	No



Nos


Lot
	
BOSE PSX1204D


BOSE DM5C


Fajar

	

	12
	System Integration

	General Requirement
The Contractor shall supply, install, integrate, configure, test, and commission a complete Audio Visual (AV) system for Meeting Room and Hybrid Meeting purposes. The proposed system shall be fully integrated and compatible with the existing AV system and shall operate seamlessly as a unified system.

System Integration with Existing AV System
The Contractor shall ensure full system integration and interoperability between the proposed AV system and the existing AV infrastructure. Integration works shall include all necessary hardware, software, interfaces, cabling, configuration, programming, and control integration to ensure seamless operation without degradation to the existing system performance.

Hybrid Meeting Functionality
The AV system shall support hybrid meeting functionality, enabling simultaneous physical and remote participation via standard video conferencing platforms (e.g. Microsoft Teams, Zoom, WebEx, or equivalent). The system shall provide clear audio, high-quality video, and stable connectivity for both local and remote participants.

Camera & Auto-Tracking System
The system shall be equipped with a live camera system with automatic speaker tracking capability. The camera shall be fully integrated with the existing microphone system to enable accurate auto-tracking based on active microphone detection. Manual override and preset camera positions shall be provided via the control system.



Audio System Integration
The proposed audio system shall be fully integrated with the existing microphone, loudspeaker, and digital signal processing (DSP) systems. Echo cancellation, noise suppression, automatic gain control, and audio mixing shall be configured to ensure optimal audio quality for hybrid meetings.

Control System
A centralized and user-friendly control interface shall be provided to allow seamless operation of all AV functions, including audio control, camera switching, source selection, display control, and hybrid meeting operation. The control system shall integrate with the existing AV control platform where applicable.


Cabling & Infrastructure
The Contractor shall supply and install all necessary outgoing cables for all AV devices, inclusive of complete cable installation works such as routing, containment, labeling, termination, and testing. All cabling works shall comply with relevant standards and best practices.

Testing & Commissioning
Comprehensive testing and commissioning shall be carried out to verify full system functionality, audio-video synchronization, auto-tracking accuracy, signal stability, and overall performance of the integrated AV system for hybrid meeting operations.



Non-Disruption to Existing System
All installation and integration works shall be carried out without disruption to the operation of the existing AV system. Any temporary shutdown or modification shall be subject to prior approval by the Client.

Documentation & Training
The Contractor shall provide complete system documentation, including as-built drawings, configuration settings, and user manuals. User training shall be conducted to ensure effective operation of the AV system for hybrid meetings.

Cost Inclusion
All AV system integration works shall be deemed included in the contract sum. No additional cost shall be borne by the Client for any works related to system integration, configuration, testing, and commissioning.

	
	
	

	13
	Warranty
	The Contractor shall provide a workmanship and service warranty for a minimum period of 12, 24 or 36 months commencing from the Date of Practical Completion / System Acceptance.

This warranty shall cover:
	•	Installation defects
	•	Cabling, termination, and finishing 		works
	•	System configuration, integration, and 		programming errors
	•	System instability caused by 			installation or configuration issues
 
Warranty Support Scope

During the warranty period, the Contractor shall provide:
	•	Technical support services.
	•	System inspection and 				troubleshooting.
	•	Repair or replacement of defective 		equipment.
	•	System reconfiguration when 			required.
	•	On-site support at no additional cost 		for issues related to the scope of work.

Response Time:
	•	Initial response within 24–48 working 		hours upon receipt of a fault report.
	•	Rectification to be carried out within a 		reasonable timeframe, subject to 			spare parts availability.

Post-Warranty Support

Upon expiry of the warranty period, the Contractor shall:
	•	Offer paid maintenance and support 		services if required.
	•	Provide quotations for repair or 			replacement of equipment

	
	
	

	14
	Value Added
	· Free 65 Inch Smart TV Panel (2 Unit)
	
	
	



BAB 4 - KETERANGAN MENGENAI KAKITANGAN & PENGALAMAN SYARIKAT

A. PROJEK YANG TELAH DILAKSANAKAN SYARIKAT

Senarai projek yang seumpama yang telah disiapkan dalam tempoh tiga tahun terakhir mengikut kronologi:-
	No.
	Butiran Kontrak
	Nama Pelanggan
dan Alamat
	Jumlah
Kontrak (RM)
	Tarikh Siap

	
	
	
	
	



B. [bookmark: _Hlk215760609][bookmark: _Hlk215760591]PROJEK YANG SEDANG DILAKSANAKAN (SEDIA ADA)

Senarai projek yang seumpama yang sedang dijalankan:-
	No.
	Butiran Kontrak
	Nama Pelanggan & Alamat
	Jumlah Kontrak (RM)
	Tarikh Mula
	Tarikh Dijangka Siap
	% Kemajuan

	
	
	
	
	
	
	





C. MAKLUMAT KAKITANGAN

1. Senarai lengkap maklumat kakitangan pengurusan syarikat. 
	NO
	NAMA (NAME)
	JAWATAN (DESIGNATION)
	BIDANG DAN TEMPOH PENGALAMAN (EXPERIENCE)
	KELAYAKAN (QUALIFICATION)

	












	
	
	
	










2. Senarai lengkap maklumat kakitangan pengurusan teknikal syarikat.
 
	NO
	NAMA (NAME)
	JAWATAN (DESIGNATION)
	BIDANG DAN TEMPOH PENGALAMAN (EXPERIENCE)
	KELAYAKAN (QUALIFICATION)

	












	
	
	
	







3. Struktur kakitangan teknikal yang akan di letakkan di bawah projek ini.

	NO
	NAMA (NAME)
	JAWATAN (DESIGNATION)
	BIDANG DAN TEMPOH PENGALAMAN (EXPERIENCE / AREA OF SUPPORT)
	TEMPOH TELAH BERKHIDMAT DGN SYARIKAT

	







.

	
(Example)

Shahril Hassan

	
(Example)

System Engineer
	
(Example)

· 3 years 
- Windows Experience
· 2 years 
- Hardware Installation  
· 1 years 
-Lotus Notes
	
(Example)

Permanent


Sila perincikan di dalam lampiran berasingan sekiranya ruang tidak mencukupi.
Sila bekalkan salinan RESUME kakitangan yang disahkan oleh majikan.



BAB 5 – JADUAL MAKLUM BALAS HARGA

	[bookmark: _Hlk221179235]Bil
	
Perkhidmatan

	Penerangan
	
Kuantiti/Lot
	
Jenama / Model
	Harga (RM)

	1
	LED Video Display with Chip on Board (COB) Technology (LEDCUBE SYSTEM P1.53-6448)

	-	LED Cabinet Size: 640mm x 480mm
-	Pixel Pitch : 1.538mm
-	Screen Size (WxH): 3.84m x 1.92m / 12.6ft x 	6.3ft
-	Screen Resolution: 2,496 x 1,248 pixels
-	LED Cabinet Array: 6 × 4 (W × H)
-	Brightness: 600-800 nits
-	Refresh rate: 3840 Hz
-	Maintenance : Front
-	LED Module Spare Unit : 5pcs
Warranty : 3 year	

Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	24 


	Nos


	
Alphal P1.53-6448-COB












	

	2
	Installation Of LED (Electrical and Civil)
	· To supply and install 30A three-phase electrical distribution board.
· To supply and install outgoing electrical cables from electrical distribution board to LED panels.
· To supply and install outgoing CAT6 cables from Video Processor to LED panels.
· To terminate all power & network cables for all LED panels.
	1 Lot
	
	

	3
	Digital Signal Processor & System Integration
	· Digital Signal Processor & System Integration camera with 20x Optical Zoom (Creator (CR-PGMIV-C).
· To supply 10.1 inch Wireless Touch Panel Screen (Apple Ipad).
· To programmable 10.1 inch Wireless Touch Panel Screen and AP Router.
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	1


1

1





	
Lot


Lot

Lot







	
Creator CR-PGMIV-C

Apple IPAD PRO
	

	4
	Project Management
	· Complete testing and commissioning.
· To supply and install all outgoing cables for all devices, inclusive of all cable installation works.
· Project Management & Consultancy.
· Project Insurance.
· User training and User Manual for all installation item.
· Installation, configuration, setup & cabling.
· Tenderers may provide any suggestions that are deemed beneficial to MIDA.
· To relocate the existing camera to another meeting room, including dismantling, reinstallation, configuration, testing, and commissioning works
· User training and User Manual on LED display operation & basic maintenance work.
	1 
	Lot
	
	

	5
	LED Display Mounting and Installation Works
	· Supply and install custom-made ceiling-mounted LED display structure. Open ceiling as needed and make good after installation.
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	1
	Lot
	
	

	6
	LED Display Control System
	· To supply and install All-in-One LED Controller 	and Processor (Novastar VX600-Pro).
· To supply and install LED Control System 	software (Novastar VX600-Pro)..
	1
	Nos
	
NovaStar VX600-PRO
	

	7
	Microphone System
	· To supply and install Full Digital Conference 	Controller Unit. 32bit high-speed DSP 	processing, audio acoustic feedback 	suppression, noise elimination (Creator CR-	DIG5201-A).
· To supply and install Digital conference 	chairman unit built-in 5.5″ wide LCD touch 	panel and adopts an embedded Linux 	operating system and is powered by an ARM 	Cortex-A7 dual-core 1.2 GHz CPU (Creator CR-	DIG5202X3).
· To supply and install Fully Digital Twisted Pair 	Conference Delegate Unit built-in loudspeaker 	c/w 415mm aviation connector plug gooseneck 	microphone with double color indicating light, 	speaking as Red color / Applying as Green 	color. Support Camera Auto -Tracking System 	function (Creator CR-CAT5204B).
· Full Digital Power Conference Extension 4 Way 	Output Box with RJ45 interfaces (Creator CR-	CAT5200-EXP-S).
· To supply and install CAT6 cable run in PVC 	conduit.
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	1




1






49







2


1
	Nos




Nos






Nos







Nos


Lot
	Creator CR-DIG5201-A



Creator CRDIG5202X3




Creator CR-Cat5204B





Creator CR-Cat5200-EXP-S
	

	8
	Camera System
	· To supply and install Camera Auto-tracking Processor which supports 6 camera Max, c/w with USB Output, Multi-View, zoom etc (Creator MID-MAX1616HD).
· To supply and install 16x8 4K Matrix Seamless Switcher Chassis as below (Creator CR-uCAT DET 4K 86:
	- 4-channel 4K HDBaseT signal seamless input
	card,Support external POC power supply 	x3pcs.
· 4-channel 4K HDMI seamless input signal card x1pc (Magewell USB Capture HDMI Plus).
· 8-channel 4K HDMI seamless output with audio signal card x2pcs (Creator CR-VX60ASL).

· HDMI, USB Type C Panel 4K HDBaseT Transmitter(150m for 1080P @60Hz, or 120m for 4K2K@60Hz 4:4:4).
· HDMI to USB 3.0 Video Capture & Streamer.


· To supply and install PTZ camera wall mount 20x Optical Zoom.
· To supply and install CAT6 cable & HDMI cable. 
Any specification that is equivalent to the stated requirement, or better, where appropriate, will be considered acceptable with justification.
	



1











11


1


3

1
	



Lot











Nos


Nos


Nos

Lot
	



Creator MID-MAX1616HD









Creator-uCAT DET 4K 86

Magewell Capture HDMI Plus
Creator CR-VX60ASL









	

	9
	Digital Signal Processor & System Integration
	·  To supply and install Digital Audio Mixer (Allen & Health CQ12T).
· Single- Ear Wireless Intercom Headset System (5 Unit).
	1
	Lot
	

Allen & Health CQ12T

	

	10
	Auxilary Display
	· To supply and install 85" Smart TV c/w wall mounted bracket (Samsung UA85CU8000).
	2
	Nos
	
Samsung UA85CU800
	

	11
	Sound / Speaker
	· To Supply and install 600 W x 4 at 8 Ω, Power Amplifier Build in DSP function (Matrix mixer, 5-band PEQ, array EQ, brand pass, Loudspeaker EQ, limiter delay).
· To supply and install 60W 5.25” Ceiling Loudspeaker.
· To supply and install 8 nos 46/0.20mm full copper speaker cable run-in PVC Conduit.
	1



8


1
	No



Nos


Lot
	
BOSE PSX1204D


BOSE DM5C


Fajar

	

	12
	System Integration

	General Requirement
The Contractor shall supply, install, integrate, configure, test, and commission a complete Audio Visual (AV) system for Meeting Room and Hybrid Meeting purposes. The proposed system shall be fully integrated and compatible with the existing AV system and shall operate seamlessly as a unified system.

System Integration with Existing AV System
The Contractor shall ensure full system integration and interoperability between the proposed AV system and the existing AV infrastructure. Integration works shall include all necessary hardware, software, interfaces, cabling, configuration, programming, and control integration to ensure seamless operation without degradation to the existing system performance.

Hybrid Meeting Functionality
The AV system shall support hybrid meeting functionality, enabling simultaneous physical and remote participation via standard video conferencing platforms (e.g. Microsoft Teams, Zoom, WebEx, or equivalent). The system shall provide clear audio, high-quality video, and stable connectivity for both local and remote participants.

Camera & Auto-Tracking System
The system shall be equipped with a live camera system with automatic speaker tracking capability. The camera shall be fully integrated with the existing microphone system to enable accurate auto-tracking based on active microphone detection. Manual override and preset camera positions shall be provided via the control system.

Audio System Integration
The proposed audio system shall be fully integrated with the existing microphone, loudspeaker, and digital signal processing (DSP) systems. Echo cancellation, noise suppression, automatic gain control, and audio mixing shall be configured to ensure optimal audio quality for hybrid meetings.

Control System
A centralized and user-friendly control interface shall be provided to allow seamless operation of all AV functions, including audio control, camera switching, source selection, display control, and hybrid meeting operation. The control system shall integrate with the existing AV control platform where applicable.

Cabling & Infrastructure
The Contractor shall supply and install all necessary outgoing cables for all AV devices, inclusive of complete cable installation works such as routing, containment, labeling, termination, and testing. All cabling works shall comply with relevant standards and best practices.

Testing & Commissioning
Comprehensive testing and commissioning shall be carried out to verify full system functionality, audio-video synchronization, auto-tracking accuracy, signal stability, and overall performance of the integrated AV system for hybrid meeting operations.



Non-Disruption to Existing System
All installation and integration works shall be carried out without disruption to the operation of the existing AV system. Any temporary shutdown or modification shall be subject to prior approval by the Client.

Documentation & Training
The Contractor shall provide complete system documentation, including as-built drawings, configuration settings, and user manuals. User training shall be conducted to ensure effective operation of the AV system for hybrid meetings.

Cost Inclusion
All AV system integration works shall be deemed included in the contract sum. No additional cost shall be borne by the Client for any works related to system integration, configuration, testing, and commissioning.

	
	
	

	13
	Warranty
	The Contractor shall provide a workmanship and service warranty for a minimum period of 12, 24 or 36 months commencing from the Date of Practical Completion / System Acceptance.

This warranty shall cover:
	•	Installation defects
	•	Cabling, termination, and finishing 		works
	•	System configuration, integration, and 		programming errors
	•	System instability caused by 			installation or configuration issues
 
Warranty Support Scope

During the warranty period, the Contractor shall provide:
	•	Technical support services.
	•	System inspection and 				troubleshooting.
	•	Repair or replacement of defective 		equipment.
	•	System reconfiguration when 			required.
	•	On-site support at no additional cost 		for issues related to the scope of work.

Response Time:
	•	Initial response within 24–48 working 		hours upon receipt of a fault report.
	•	Rectification to be carried out within a 		reasonable timeframe, subject to 			spare parts availability.

Post-Warranty Support

Upon expiry of the warranty period, the Contractor shall:
	•	Offer paid maintenance and support 		services if required.
	•	Provide quotations for repair or 			replacement of equipment

	
	
	

	14
	Value Added
	· Free 65 Inch Smart TV Panel (2 Unit)
	
	
	

	15
	HARGA (RM)
	

	16
	CUKAI PERKHIDMATAN DAN JUALAN (SST)
	

	17
	HARGA KESELURUHAN (RM)
	



BAB 6

BUTIR-BUTIR PENYEBUTHARGA & MAKLUMAT KEWANGAN SYARIKAT


Syarikat perlu mengisi dengan lengkap semua seksyen dalam borang ini. Sekiranya ruang tidak mencukupi, maklumat boleh dikemukakan dalam kertas berasingan.

A.	MAKLUMAT AM

	1. 
	Nama Syarikat
	:
	

	2. 
	Alamat
	:
	

	3. 
	No. Telefon
	:
	

	4. 
	No. Faks
	:
	

	5. 
	Emel
	:
	

	6. 
	Tarikh Pendaftaran / Penubuhan
	:
	

	7. 
	No. Daftar Syarikat / Perniagaan
	:
	

	8. 
	Tempat Pendaftaran/ Penubuhan
	:
	

	9. 
	Komposisi Pemegang Saham
	:
	

	
	No.
	Nama Pemegang Saham
	Jawatan
	% Pegangan

	
	
	
	
	



10. Peratusan Penyertaan Bumiputera : ________ (%). (Sila kemukakan maklumat lanjut atau salinan sah pendaftaran sebagai Pembekal Bumiputera dengan Kementerian Kewangan).

11. Maklumat Pendaftaran Kementerian Kewangan

	No.
	No. Pendaftaran
	No. bidang
	Butiran / Keterangan
	Tempoh Sah

	
	
	
	
	

	
	
	
	
	



Nota : Sila lampirkan salinan sijil pendaftaran.

12.	Struktur Modal Syarikat :

	(i) Modal Dibenarkan

	:

	(ii) Modal Berbayar

	:








B.	KEWANGAN

a.	Ringkasan aset dan tanggungan berdasarkan akaun yang diaudit bagi tiga (3) tahun terakhir.

	Tahun Kewangan:
	2023
(RM)
	2024
(RM)
	2025
(RM)

	· Jumlah Aset 
· Aset Semasa 
· Jumlah Tanggungan 
· Tanggungan Semasa 
· Nilai Bersih 
· Modal Kerja 
	
	
	




b. Bank-bank Utama:

	No.
	Nama Bank & Alamat
	Jenis Akaun

	1.
2.
3.
	
	





c. Kemudahan Kredit (Jenis dan jumlah kredit yang boleh disediakan oleh syarikat:)

	No.
	Jenis Kemudahan Kredit
	Bank/Institusi Kewangan
	Jumlah (RM)

	1.
2.
3.
	
	
	



Nota:
1. Penyata Kewangan yang telah diaudit bagi tempoh tiga (3) tahun terakhir hendaklah disertakan bersama-sama serahan borang sebutharga.
2. Penyata Bank bagi tempoh tiga (3) bulan terakhir hendaklah disertakan bersama-sama serahan borang sebutharga.





LAMPIRAN SEMAKAN

SEBUTHARGA KERJA-KERJA MENAIKTARAF SISTEM AUDIO VISUAL DI BILIK MESYUARAT JAPAN, TINGKAT 18, MIDA SENTRAL

SEBUTHARGA MIDA BIL: 19/2026

Sila tandakan ( √ ) bagi Dokumen-dokumen yang disertakan.

	Bil.
	Perkara / Dokumen
	Semakan oleh Syarikat
	Semakan oleh 
MIDA

	1. 
	Surat Akuan Penyebutharga*
	
	

	2. 
	Surat Akuan Pembida*
	
	

	3. 
	Maklumat Suruhanjaya Syarikat Malaysia (SSM) (Salinan sijil disertakan)
	
	

	
	Berdaftar dengan SSM* 
	
	

	
	i) No. Sijil Pendaftaran (sila nyatakan)
	
	

	
	ii) Tempoh Sahlaku Sijil Pendaftaran (nyatakan)
	
	

	4. 
	Maklumat pendaftaran dengan Kementerian Kewangan (MOF) (Salinan Sijil Akuan Pendaftaran dengan MOF disertakan)
	
	

	
	Syarikat berdaftar dengan Kementerian Kewangan (MOF)* dalam kod bidang berikut (dan tempoh pendaftaran masih berkuatkuasa):

020302 – Perkakas Elektronik dan Aksesori; ATAU
221304 – Audio Visual; DAN / ATAU
222601 – Akustik dan Gelombang

	
	

	
	i) No. Sijil Akuan Pendaftaran (nyatakan)
	
	

	
	ii) Tempoh Sahlaku Sijil Pendaftaran (nyatakan)
	
	

	
	iii) Salinan Sijil disertakan
	
	

	
	iv) Sijil Akuan Pendaftaran Bumiputera (jika ada)
	
	

	
	v) Peratus Penyertaan/Ekuiti Bumiputera (nyatakan, jika ada)
	
	

	5.
	Syarikat mengemukakan Sijil Pematuhan Cukai (TCC)*
	
	

	6.
	Jadual Maklumbalas Teknikal (Hardcopy & Softcopy)
	
	

	7.	Jadual Maklumbalas Harga (Hardcopy & Softcopy)
	
	

	
	i) Borang Jadual Harga
	
	

	
	ii) Penyata Kewangan (yang telah diaudit) untuk 3 tahun terakhir
	
	

	
	iii) Penyata Bank untuk 3 bulan terakhir
	
	

	8.
	Lain-lain seperti:-
· Latar belakang syarikat / Executive Summary
· Carta organisasi syarikat
· Project Implementation Plan
	
	

	9.
	[bookmark: _heading=h.1dw4iungjt8r]Pengesahan Oleh Syarikat*
	
	


 *Mandatori

	PENGESAHAN OLEH SYARIKAT


	Dengan ini saya mengesahkan bahawa saya telah membaca dan memahami semua syarat-syarat dan terma yang dinyatakan di dalam dokumen sebut harga. Semua maklumat yang dikemukakan adalah benar.


	
	Tandatangan
	:
	.....................................................................................


	Nama
	:
	.....................................................................................


	Jawatan
	:
	.....................................................................................


	Tarikh
	:
	.....................................................................................







	PENGESAHAN OLEH MIDA


	Jawatankuasa Penilaian Sebutharga mengesahkan penerimaan dokumen bertanda kecuali bagi perkara bil. .......................................... (jika ada) :-


	
	Tandatangan
	:
	.....................................................................................


	Nama
	:
	.....................................................................................


	Jawatan
	:
	.....................................................................................


	Tarikh
	:
	.....................................................................................







